=== Interface IPv6 autoconf for bridges

ifdef::topdoc[:imagesdir: {topdoc}../../test/case/interfaces/ipv6_address]

==== Description

Verify IPv6 autoconf on a bridge is properly set up for global prefix.
See issue #473 for details.

==== Topology

image::topology.svg[Interface IPv6 autoconf for bridges topology, align=center, scaledwidth=75%]

==== Sequence

. Set up topology and attach to target DUT
. Setting up bridge with IPv6 SLAAC for global prefix on target:data
. Verify using sysctl that 'net.ipv6.conf.br0.autoconf' is 1 on target


