=== Bridge with a physical port and a veth

ifdef::topdoc[:imagesdir: {topdoc}../../test/case/interfaces/bridge_veth]

==== Description

This tests the possibility to add software added interfaces, in this case
VETH and bridge it with a physical interface

....

PING -->      br0
             /   \
 PC- target:data  veth0a -- veth0b
     10.0.0.1               10.0.0.2

....

==== Topology

image::topology.svg[Bridge with a physical port and a veth topology, align=center, scaledwidth=75%]

==== Sequence

. Set up topology and attach to target DUT
. Configure bridged eth port and veth pair with IP 10.0.0.2
. Verify ping from host:data to 10.0.0.2


