name                : br-D
type                : bridge
index               : 15
mtu                 : 1500
operational status  : up
ip forwarding       : disabled
physical address    : 00:a0:85:00:03:00
ipv4 addresses      : 10.0.0.1/8 (static)
                      192.168.20.1/24 (static)
ipv6 addresses      : 2001:db8::1/64 (static)
                      fe80::2a0:85ff:fe00:300/64 (link-layer)
