/* Upstream device trees specify regular PSCI support for SparX-5i,
 * but the U-Boot that Microchip ships does not actually support it.
 * Therefore, wrap the upstream version to disable PSCI and revert to
 * spin tables for SMP bringup.
 */

/dts-v1/;
#include <arm64/microchip/sparx5_pcb135_emmc.dts>

&cpu0 {
	enable-method = "spin-table";
	cpu-release-addr = <0x0 0x0000fff8>;
};

&cpu1 {
	enable-method = "spin-table";
	cpu-release-addr = <0x0 0x0000fff8>;
};

/ {
	/delete-node/ psci;
};
