=== Interface Description (ifAlias)
==== Description
Verify interface description (ifAlias) can be set on an interface and
then be read back from the operational datastore.

==== Topology
ifdef::topdoc[]
image::{topdoc}../../test/case/ietf_interfaces/ifalias/topology.svg[Interface Description (ifAlias) topology]
endif::topdoc[]
ifndef::topdoc[]
ifdef::testgroup[]
image::ifalias/topology.svg[Interface Description (ifAlias) topology]
endif::testgroup[]
ifndef::testgroup[]
image::topology.svg[Interface Description (ifAlias) topology]
endif::testgroup[]
endif::topdoc[]
==== Test sequence
. Set up topology and attach to target DUT
. Set up interface target:data with description
. Verify description can be read back from operational


<<<

