=== Interface IPv6 autoconf for bridges
==== Description
Verify IPv6 autoconf on a bridge is properly set up for global prefix.
See issue #473 for details.

==== Topology
ifdef::topdoc[]
image::{topdoc}../../test/case/ietf_interfaces/ipv6_address/topology.svg[Interface IPv6 autoconf for bridges topology]
endif::topdoc[]
ifndef::topdoc[]
ifdef::testgroup[]
image::ipv6_address/topology.svg[Interface IPv6 autoconf for bridges topology]
endif::testgroup[]
ifndef::testgroup[]
image::topology.svg[Interface IPv6 autoconf for bridges topology]
endif::testgroup[]
endif::topdoc[]
==== Test sequence
. Set up topology and attach to target DUT
. Setting up bridge with IPv6 SLAAC for global prefix on target:data
. Verify using sysctl that 'net.ipv6.conf.br0.autoconf' is 1 on target


<<<

