=== VXLAN bridged with physical interface
==== Description
Test that vxlan works as it should and that it possible to bridge it.

==== Topology
ifdef::topdoc[]
image::{topdoc}../../test/case/ietf_interfaces/tunnel_bridged/topology.svg[VXLAN bridged with physical interface topology]
endif::topdoc[]
ifndef::topdoc[]
ifdef::testgroup[]
image::tunnel_bridged/topology.svg[VXLAN bridged with physical interface topology]
endif::testgroup[]
ifndef::testgroup[]
image::topology.svg[VXLAN bridged with physical interface topology]
endif::testgroup[]
endif::topdoc[]
==== Test sequence
. Set up topology and attach to target DUTs
. Configure DUTs
. Test connectivity host:data to right:vxlan0 at 192.168.10.2


<<<

