=== Static routing
==== Description
Verify that it is possible to add static routes, both IPv4 and IPv6, and
that data forwarding works as expected via an intermediate device.

==== Topology
ifdef::topdoc[]
image::{topdoc}../../test/case/ietf_routing/static_routing/topology.svg[Static routing topology]
endif::topdoc[]
ifndef::topdoc[]
ifdef::testgroup[]
image::static_routing/topology.svg[Static routing topology]
endif::testgroup[]
ifndef::testgroup[]
image::topology.svg[Static routing topology]
endif::testgroup[]
endif::topdoc[]
==== Test sequence
. Set up topology and attach to target DUTs
. Configure targets
. Wait for routes
. Configure host addresses and routes
. Verify that R2 is reachable on 192.168.200.1 from PC:data
. Verify that R2 is reachable on 2001:db8:3c4d:200::1 from PC:data
. Remove all static routes from R1
. Verify R2 is no longer reachable on either IPv4 or IPv6 from PC:data


<<<

