=== Bridge basic
==== Description
Test basic connectivity to a bridge

....

    PING -->                br0 (10.0.0.2)
                            /
    PC -------- target:data

....

==== Topology
ifdef::topdoc[]
image::{topdoc}../../test/case/ietf_interfaces/bridge_basic/topology.svg[Bridge basic topology]
endif::topdoc[]
ifndef::topdoc[]
ifdef::testgroup[]
image::bridge_basic/topology.svg[Bridge basic topology]
endif::testgroup[]
ifndef::testgroup[]
image::topology.svg[Bridge basic topology]
endif::testgroup[]
endif::topdoc[]
==== Test sequence
. Set up topology and attach to target DUT
. Configure single bridge with a single physical port, bridge @ IP 10.0.0.2
. Verify ping 10.0.0.2 is possible from host:data


<<<

