=== Container with physical interface
==== Description
Verify connectivity with a simple web server container that's been
given a physical interface instead of an end of a VETH pair.

==== Topology
ifdef::topdoc[]
image::{topdoc}../../test/case/infix_containers/container_phys/topology.svg[Container with physical interface topology]
endif::topdoc[]
ifndef::topdoc[]
ifdef::testgroup[]
image::container_phys/topology.svg[Container with physical interface topology]
endif::testgroup[]
ifndef::testgroup[]
image::topology.svg[Container with physical interface topology]
endif::testgroup[]
endif::topdoc[]
==== Test sequence
. Set up topology and attach to target DUT
. Create httpd container from bundled OCI image
. Verify container has started
. Verify host:data can ping 10.0.0.2
. Verify container is reachable on http://10.0.0.2:91
. Add a content mount, overriding index.html
. Verify server is restarted and returns new content


<<<

