=== Bridge VLAN
==== Description
Verify VLAN filtering bridge, with a VLAN trunk to a neighboring device,
which in turn untags one VLAN outisde a non-VLAN filtering bridge.

.Logical network setup
ifdef::topdoc[]
image::{topdoc}../../test/case/ietf_interfaces/bridge_vlan/bridge-vlan.svg[]
endif::topdoc[]
ifndef::topdoc[]
ifdef::testgroup[]
image::bridge_vlan/bridge-vlan.svg[]
endif::testgroup[]
ifndef::testgroup[]
image::bridge-vlan.svg[]
endif::testgroup[]
endif::topdoc[]

==== Topology
ifdef::topdoc[]
image::{topdoc}../../test/case/ietf_interfaces/bridge_vlan/topology.svg[Bridge VLAN topology]
endif::topdoc[]
ifndef::topdoc[]
ifdef::testgroup[]
image::bridge_vlan/topology.svg[Bridge VLAN topology]
endif::testgroup[]
ifndef::testgroup[]
image::topology.svg[Bridge VLAN topology]
endif::testgroup[]
endif::topdoc[]
==== Test sequence
. Set up topology and attach to target DUT
. Configure DUTs
. Verify ping from host:data to 10.0.0.2 and 10.0.0.3


<<<

