=== Routing basic
==== Description
Verify routing between interfaces is possible. That enable/disable routing
in configuration has the expected result.

==== Topology
ifdef::topdoc[]
image::{topdoc}../../test/case/ietf_interfaces/routing_basic/topology.svg[Routing basic topology]
endif::topdoc[]
ifndef::topdoc[]
ifdef::testgroup[]
image::routing_basic/topology.svg[Routing basic topology]
endif::testgroup[]
ifndef::testgroup[]
image::topology.svg[Routing basic topology]
endif::testgroup[]
endif::topdoc[]
==== Test sequence
. Set up topology and attach to target DUTs
. Setup host
. Enable forwarding on target:data1 and target:data2
. Verify ping from host:data1 to 10.0.0.10
. Verify ping from host:data2 to 192.168.0.10
. Disable forwarding on target:data1 and target:data2
. Verify ping does not work host:data1 to 10.0.0.10 and host:data2 to 192.168.0.10


<<<

