=== Dual bridges on one device
==== Description
Verify that it is possible to ping through a bridge to another bridge via VETH interfaces.

....
 PING -->     br0             br1 10.0.0.2
             /   \              /
PC - target:data  veth0a - veth0b
....

==== Topology
ifdef::topdoc[]
image::{topdoc}../../test/case/ietf_interfaces/dual_bridge/topology.svg[Dual bridges on one device topology]
endif::topdoc[]
ifndef::topdoc[]
ifdef::testgroup[]
image::dual_bridge/topology.svg[Dual bridges on one device topology]
endif::testgroup[]
ifndef::testgroup[]
image::topology.svg[Dual bridges on one device topology]
endif::testgroup[]
endif::topdoc[]
==== Test sequence
. Set up topology and attach to target DUTs
. Configure two bridges linked and a veth pair
. Verify ping from host:data to 10.0.0.2


<<<

