[7mINTERFACE       PROTOCOL   STATE       DATA                                     [0m
lo              loopback   [32mUP          [39m
                ipv4                   127.0.0.1/8 (static)
                ipv6                   ::1/128 (static)
br0             bridge     [33m            [39mvlan:1u pvid:1                           
│               ethernet   [32mUP          [39m00:a0:85:00:03:00                        
│               ipv4                   169.254.1.1/16 (random)
│               ipv6                   fe80::2a0:85ff:fe00:300/64 (link-layer)
├ e3            bridge     [32mFORWARDING  [39mvlan:1u pvid:1                           
├ e4            bridge     [32mFORWARDING  [39mvlan:1u pvid:1                           
├ veth0b        bridge     [32mFORWARDING  [39mvlan:1u pvid:1                           
└ veth2b        bridge     [32mFORWARDING  [39mvlan:1u pvid:1                           
br1             bridge     [33m            [39m
│               ethernet   [32mUP          [39m00:a0:85:00:03:00                        
├ veth1b        bridge     [32mFORWARDING  [39mvlan:6u pvid:6                           
└ veth3b        bridge     [32mFORWARDING  [39m
e1              ethernet   [32mUP          [39m00:a0:85:00:03:01                        
                ipv6                   fe80::2a0:85ff:fe00:301/64 (link-layer)
e2              ethernet   [32mUP          [39m00:a0:85:00:03:02                        
                ipv6                   fe80::2a0:85ff:fe00:302/64 (link-layer)
e3.8            ethernet   [32mUP          [39m00:a0:85:00:03:03                        
│               ipv4                   10.1.1.1/32 (static)
└ e3            ethernet   [32mUP          [39m00:a0:85:00:03:03                        
e4.8            ethernet   [32mUP          [39m00:a0:85:00:03:04                        
│               ipv4                   10.1.1.1/32 (static)
└ e4            ethernet   [32mUP          [39m00:a0:85:00:03:04                        
e5              ethernet   [32mUP          [39m00:a0:85:00:03:05                        
                ipv6                   fe80::2a0:85ff:fe00:305/64 (link-layer)
e6              ethernet   [32mUP          [39m00:a0:85:00:03:06                        
                ipv4                   10.1.1.101/24 (static)
                ipv6                   fe80::2a0:85ff:fe00:306/64 (link-layer)
e7              ethernet   [32mUP          [39m00:a0:85:00:03:07                        
                ipv6                   fe80::2a0:85ff:fe00:307/64 (link-layer)
[100mveth0a          container              container-A                              [0m
veth0b          veth       [32mUP          [39me6:19:75:86:80:dd                        
[100mveth1a          container              container-A                              [0m
veth1b          veth       [32mUP          [39m3e:67:0f:15:24:14                        
[100mveth2a          container              container-B                              [0m
veth2b          veth       [32mUP          [39mb2:fa:30:63:98:f0                        
[100mveth3a          container              container-B                              [0m
veth3b          veth       [32mUP          [39mb2:1c:fa:a7:45:eb                        
