From 312d3efde0fbe7cec3bf7ba1908c213c9cf69337 Mon Sep 17 00:00:00 2001
From: Andrew Lunn <andrew@lunn.ch>
Date: Tue, 8 Aug 2023 23:04:33 +0200
Subject: [PATCH 10/17] led: trig: netdev: Fix requesting offload device

When the netdev trigger is activates, it tries to determine what
device the LED blinks for, and what the current blink mode is.

The documentation for hw_control_get() says:

	 * Return 0 on success, a negative error number on failing parsing the
	 * initial mode. Error from this function is NOT FATAL as the device
	 * may be in a not supported initial state by the attached LED trigger.
	 */

For the Marvell PHY and the Armada 370-rd board, the initial LED blink
mode is not supported by the trigger, so it returns an error. This
resulted in not getting the device the LED is blinking for. As a
result, the device is unknown and offloaded is never performed.

Change to condition to always get the device if offloading is
supported, and reduce the scope of testing for an error from
hw_control_get() to skip setting trigger internal state if there is an
error.

Reviewed-by: Simon Horman <simon.horman@corigine.com>
Signed-off-by: Andrew Lunn <andrew@lunn.ch>
Tested-by: Daniel Golle <daniel@makrotopia.org>
Link: https://lore.kernel.org/r/20230808210436.838995-2-andrew@lunn.ch
Signed-off-by: Jakub Kicinski <kuba@kernel.org>
Signed-off-by: Tobias Waldekranz <tobias@waldekranz.com>
---
 drivers/leds/trigger/ledtrig-netdev.c | 8 +++++---
 1 file changed, 5 insertions(+), 3 deletions(-)

diff --git a/drivers/leds/trigger/ledtrig-netdev.c b/drivers/leds/trigger/ledtrig-netdev.c
index 03c58e50cc44..e9e4da217249 100644
--- a/drivers/leds/trigger/ledtrig-netdev.c
+++ b/drivers/leds/trigger/ledtrig-netdev.c
@@ -564,15 +564,17 @@ static int netdev_trig_activate(struct led_classdev *led_cdev)
 	/* Check if hw control is active by default on the LED.
 	 * Init already enabled mode in hw control.
 	 */
-	if (supports_hw_control(led_cdev) &&
-	    !led_cdev->hw_control_get(led_cdev, &mode)) {
+	if (supports_hw_control(led_cdev)) {
 		dev = led_cdev->hw_control_get_device(led_cdev);
 		if (dev) {
 			const char *name = dev_name(dev);
 
 			set_device_name(trigger_data, name, strlen(name));
 			trigger_data->hw_control = true;
-			trigger_data->mode = mode;
+
+			rc = led_cdev->hw_control_get(led_cdev, &mode);
+			if (!rc)
+				trigger_data->mode = mode;
 		}
 	}
 
-- 
2.34.1

