From 1d6f30fce9f4516730439f72ee2134301d37654d Mon Sep 17 00:00:00 2001
From: Tobias Waldekranz <tobias@waldekranz.com>
Date: Tue, 5 Sep 2023 13:08:29 +0200
Subject: [PATCH 02/17] net: dsa: mv88e6xxx: Create API to read a single stat
 counter

This change contains no functional change. We simply push the hardware
specific stats logic to a function reading a single counter, rather
than the whole set.

This is a preparatory change for the upcoming standard ethtool
statistics support (i.e. "eth-mac", "eth-ctrl" etc.).

Signed-off-by: Tobias Waldekranz <tobias@waldekranz.com>
---
 drivers/net/dsa/mv88e6xxx/chip.c | 160 ++++++++++++++++++-------------
 drivers/net/dsa/mv88e6xxx/chip.h |  27 +++---
 2 files changed, 105 insertions(+), 82 deletions(-)

diff --git a/drivers/net/dsa/mv88e6xxx/chip.c b/drivers/net/dsa/mv88e6xxx/chip.c
index 0d4b236d1e34..139f4d55a284 100644
--- a/drivers/net/dsa/mv88e6xxx/chip.c
+++ b/drivers/net/dsa/mv88e6xxx/chip.c
@@ -1082,7 +1082,7 @@ static struct mv88e6xxx_hw_stat mv88e6xxx_hw_stats[] = {
 };
 
 static uint64_t _mv88e6xxx_get_ethtool_stat(struct mv88e6xxx_chip *chip,
-					    struct mv88e6xxx_hw_stat *s,
+					    const struct mv88e6xxx_hw_stat *s,
 					    int port, u16 bank1_select,
 					    u16 histogram)
 {
@@ -1265,59 +1265,82 @@ static int mv88e6xxx_get_sset_count(struct dsa_switch *ds, int port, int sset)
 	return count;
 }
 
-static int mv88e6xxx_stats_get_stats(struct mv88e6xxx_chip *chip, int port,
-				     uint64_t *data, int types,
-				     u16 bank1_select, u16 histogram)
+static int mv88e6095_stats_get_stat(struct mv88e6xxx_chip *chip, int port,
+				    const struct mv88e6xxx_hw_stat *stat,
+				    uint64_t *data)
 {
-	struct mv88e6xxx_hw_stat *stat;
-	int i, j;
+	if (!(stat->type & (STATS_TYPE_BANK0 | STATS_TYPE_PORT)))
+		return 0;
 
-	for (i = 0, j = 0; i < ARRAY_SIZE(mv88e6xxx_hw_stats); i++) {
-		stat = &mv88e6xxx_hw_stats[i];
-		if (stat->type & types) {
-			mv88e6xxx_reg_lock(chip);
-			data[j] = _mv88e6xxx_get_ethtool_stat(chip, stat, port,
-							      bank1_select,
-							      histogram);
-			mv88e6xxx_reg_unlock(chip);
+	*data = _mv88e6xxx_get_ethtool_stat(chip, stat, port, 0,
+					    MV88E6XXX_G1_STATS_OP_HIST_RX_TX);
+	return 1;
+}
 
-			j++;
-		}
-	}
-	return j;
+static int mv88e6250_stats_get_stat(struct mv88e6xxx_chip *chip, int port,
+				    const struct mv88e6xxx_hw_stat *stat,
+				    uint64_t *data)
+{
+	if (!(stat->type & STATS_TYPE_BANK0))
+		return 0;
+
+	*data = _mv88e6xxx_get_ethtool_stat(chip, stat, port, 0,
+					    MV88E6XXX_G1_STATS_OP_HIST_RX_TX);
+	return 1;
 }
 
-static int mv88e6095_stats_get_stats(struct mv88e6xxx_chip *chip, int port,
-				     uint64_t *data)
+static int mv88e6320_stats_get_stat(struct mv88e6xxx_chip *chip, int port,
+				    const struct mv88e6xxx_hw_stat *stat,
+				    uint64_t *data)
 {
-	return mv88e6xxx_stats_get_stats(chip, port, data,
-					 STATS_TYPE_BANK0 | STATS_TYPE_PORT,
-					 0, MV88E6XXX_G1_STATS_OP_HIST_RX_TX);
+	if (!(stat->type & (STATS_TYPE_BANK0 | STATS_TYPE_BANK1)))
+		return 0;
+
+	*data = _mv88e6xxx_get_ethtool_stat(chip, stat, port,
+					    MV88E6XXX_G1_STATS_OP_BANK_1_BIT_9,
+					    MV88E6XXX_G1_STATS_OP_HIST_RX_TX);
+	return 1;
 }
 
-static int mv88e6250_stats_get_stats(struct mv88e6xxx_chip *chip, int port,
-				     uint64_t *data)
+static int mv88e6390_stats_get_stat(struct mv88e6xxx_chip *chip, int port,
+				    const struct mv88e6xxx_hw_stat *stat,
+				    uint64_t *data)
 {
-	return mv88e6xxx_stats_get_stats(chip, port, data, STATS_TYPE_BANK0,
-					 0, MV88E6XXX_G1_STATS_OP_HIST_RX_TX);
+	if (!(stat->type & (STATS_TYPE_BANK0 | STATS_TYPE_BANK1)))
+		return 0;
+
+	*data = _mv88e6xxx_get_ethtool_stat(chip, stat, port,
+					    MV88E6XXX_G1_STATS_OP_BANK_1_BIT_10,
+					    0);
+	return 1;
 }
 
-static int mv88e6320_stats_get_stats(struct mv88e6xxx_chip *chip, int port,
-				     uint64_t *data)
+static int mv88e6xxx_stats_get_stat(struct mv88e6xxx_chip *chip, int port,
+				    const struct mv88e6xxx_hw_stat *stat,
+				    uint64_t *data)
 {
-	return mv88e6xxx_stats_get_stats(chip, port, data,
-					 STATS_TYPE_BANK0 | STATS_TYPE_BANK1,
-					 MV88E6XXX_G1_STATS_OP_BANK_1_BIT_9,
-					 MV88E6XXX_G1_STATS_OP_HIST_RX_TX);
+	int ret = 0;
+
+	if (chip->info->ops->stats_get_stat) {
+		mv88e6xxx_reg_lock(chip);
+		ret = chip->info->ops->stats_get_stat(chip, port, stat, data);
+		mv88e6xxx_reg_unlock(chip);
+	}
+
+	return ret;
 }
 
-static int mv88e6390_stats_get_stats(struct mv88e6xxx_chip *chip, int port,
+static int mv88e6xxx_stats_get_stats(struct mv88e6xxx_chip *chip, int port,
 				     uint64_t *data)
 {
-	return mv88e6xxx_stats_get_stats(chip, port, data,
-					 STATS_TYPE_BANK0 | STATS_TYPE_BANK1,
-					 MV88E6XXX_G1_STATS_OP_BANK_1_BIT_10,
-					 0);
+	struct mv88e6xxx_hw_stat *stat;
+	int i, j;
+
+	for (i = 0, j = 0; i < ARRAY_SIZE(mv88e6xxx_hw_stats); i++) {
+		stat = &mv88e6xxx_hw_stats[i];
+		j += mv88e6xxx_stats_get_stat(chip, port, stat, &data[j]);
+	}
+	return j;
 }
 
 static void mv88e6xxx_atu_vtu_get_stats(struct mv88e6xxx_chip *chip, int port,
@@ -1333,10 +1356,9 @@ static void mv88e6xxx_atu_vtu_get_stats(struct mv88e6xxx_chip *chip, int port,
 static void mv88e6xxx_get_stats(struct mv88e6xxx_chip *chip, int port,
 				uint64_t *data)
 {
-	int count = 0;
+	int count;
 
-	if (chip->info->ops->stats_get_stats)
-		count = chip->info->ops->stats_get_stats(chip, port, data);
+	count = mv88e6xxx_stats_get_stats(chip, port, data);
 
 	mv88e6xxx_reg_lock(chip);
 	if (chip->info->ops->serdes_get_stats) {
@@ -4198,7 +4220,7 @@ static const struct mv88e6xxx_ops mv88e6085_ops = {
 	.stats_set_histogram = mv88e6095_g1_stats_set_histogram,
 	.stats_get_sset_count = mv88e6095_stats_get_sset_count,
 	.stats_get_strings = mv88e6095_stats_get_strings,
-	.stats_get_stats = mv88e6095_stats_get_stats,
+	.stats_get_stat = mv88e6095_stats_get_stat,
 	.set_cpu_port = mv88e6095_g1_set_cpu_port,
 	.set_egress_port = mv88e6095_g1_set_egress_port,
 	.watchdog_ops = &mv88e6097_watchdog_ops,
@@ -4236,7 +4258,7 @@ static const struct mv88e6xxx_ops mv88e6095_ops = {
 	.stats_set_histogram = mv88e6095_g1_stats_set_histogram,
 	.stats_get_sset_count = mv88e6095_stats_get_sset_count,
 	.stats_get_strings = mv88e6095_stats_get_strings,
-	.stats_get_stats = mv88e6095_stats_get_stats,
+	.stats_get_stat = mv88e6095_stats_get_stat,
 	.mgmt_rsvd2cpu = mv88e6185_g2_mgmt_rsvd2cpu,
 	.serdes_power = mv88e6185_serdes_power,
 	.serdes_get_lane = mv88e6185_serdes_get_lane,
@@ -4279,7 +4301,7 @@ static const struct mv88e6xxx_ops mv88e6097_ops = {
 	.stats_set_histogram = mv88e6095_g1_stats_set_histogram,
 	.stats_get_sset_count = mv88e6095_stats_get_sset_count,
 	.stats_get_strings = mv88e6095_stats_get_strings,
-	.stats_get_stats = mv88e6095_stats_get_stats,
+	.stats_get_stat = mv88e6095_stats_get_stat,
 	.set_cpu_port = mv88e6095_g1_set_cpu_port,
 	.set_egress_port = mv88e6095_g1_set_egress_port,
 	.watchdog_ops = &mv88e6097_watchdog_ops,
@@ -4325,7 +4347,7 @@ static const struct mv88e6xxx_ops mv88e6123_ops = {
 	.stats_set_histogram = mv88e6095_g1_stats_set_histogram,
 	.stats_get_sset_count = mv88e6095_stats_get_sset_count,
 	.stats_get_strings = mv88e6095_stats_get_strings,
-	.stats_get_stats = mv88e6095_stats_get_stats,
+	.stats_get_stat = mv88e6095_stats_get_stat,
 	.set_cpu_port = mv88e6095_g1_set_cpu_port,
 	.set_egress_port = mv88e6095_g1_set_egress_port,
 	.watchdog_ops = &mv88e6097_watchdog_ops,
@@ -4368,7 +4390,7 @@ static const struct mv88e6xxx_ops mv88e6131_ops = {
 	.stats_set_histogram = mv88e6095_g1_stats_set_histogram,
 	.stats_get_sset_count = mv88e6095_stats_get_sset_count,
 	.stats_get_strings = mv88e6095_stats_get_strings,
-	.stats_get_stats = mv88e6095_stats_get_stats,
+	.stats_get_stat = mv88e6095_stats_get_stat,
 	.set_cpu_port = mv88e6095_g1_set_cpu_port,
 	.set_egress_port = mv88e6095_g1_set_egress_port,
 	.watchdog_ops = &mv88e6097_watchdog_ops,
@@ -4417,7 +4439,7 @@ static const struct mv88e6xxx_ops mv88e6141_ops = {
 	.stats_set_histogram = mv88e6390_g1_stats_set_histogram,
 	.stats_get_sset_count = mv88e6320_stats_get_sset_count,
 	.stats_get_strings = mv88e6320_stats_get_strings,
-	.stats_get_stats = mv88e6390_stats_get_stats,
+	.stats_get_stat = mv88e6390_stats_get_stat,
 	.set_cpu_port = mv88e6390_g1_set_cpu_port,
 	.set_egress_port = mv88e6390_g1_set_egress_port,
 	.watchdog_ops = &mv88e6390_watchdog_ops,
@@ -4479,7 +4501,7 @@ static const struct mv88e6xxx_ops mv88e6161_ops = {
 	.stats_set_histogram = mv88e6095_g1_stats_set_histogram,
 	.stats_get_sset_count = mv88e6095_stats_get_sset_count,
 	.stats_get_strings = mv88e6095_stats_get_strings,
-	.stats_get_stats = mv88e6095_stats_get_stats,
+	.stats_get_stat = mv88e6095_stats_get_stat,
 	.set_cpu_port = mv88e6095_g1_set_cpu_port,
 	.set_egress_port = mv88e6095_g1_set_egress_port,
 	.watchdog_ops = &mv88e6097_watchdog_ops,
@@ -4517,7 +4539,7 @@ static const struct mv88e6xxx_ops mv88e6165_ops = {
 	.stats_set_histogram = mv88e6095_g1_stats_set_histogram,
 	.stats_get_sset_count = mv88e6095_stats_get_sset_count,
 	.stats_get_strings = mv88e6095_stats_get_strings,
-	.stats_get_stats = mv88e6095_stats_get_stats,
+	.stats_get_stat = mv88e6095_stats_get_stat,
 	.set_cpu_port = mv88e6095_g1_set_cpu_port,
 	.set_egress_port = mv88e6095_g1_set_egress_port,
 	.watchdog_ops = &mv88e6097_watchdog_ops,
@@ -4565,7 +4587,7 @@ static const struct mv88e6xxx_ops mv88e6171_ops = {
 	.stats_set_histogram = mv88e6095_g1_stats_set_histogram,
 	.stats_get_sset_count = mv88e6095_stats_get_sset_count,
 	.stats_get_strings = mv88e6095_stats_get_strings,
-	.stats_get_stats = mv88e6095_stats_get_stats,
+	.stats_get_stat = mv88e6095_stats_get_stat,
 	.set_cpu_port = mv88e6095_g1_set_cpu_port,
 	.set_egress_port = mv88e6095_g1_set_egress_port,
 	.watchdog_ops = &mv88e6097_watchdog_ops,
@@ -4614,7 +4636,7 @@ static const struct mv88e6xxx_ops mv88e6172_ops = {
 	.stats_set_histogram = mv88e6095_g1_stats_set_histogram,
 	.stats_get_sset_count = mv88e6095_stats_get_sset_count,
 	.stats_get_strings = mv88e6095_stats_get_strings,
-	.stats_get_stats = mv88e6095_stats_get_stats,
+	.stats_get_stat = mv88e6095_stats_get_stat,
 	.set_cpu_port = mv88e6095_g1_set_cpu_port,
 	.set_egress_port = mv88e6095_g1_set_egress_port,
 	.watchdog_ops = &mv88e6097_watchdog_ops,
@@ -4670,7 +4692,7 @@ static const struct mv88e6xxx_ops mv88e6175_ops = {
 	.stats_set_histogram = mv88e6095_g1_stats_set_histogram,
 	.stats_get_sset_count = mv88e6095_stats_get_sset_count,
 	.stats_get_strings = mv88e6095_stats_get_strings,
-	.stats_get_stats = mv88e6095_stats_get_stats,
+	.stats_get_stat = mv88e6095_stats_get_stat,
 	.set_cpu_port = mv88e6095_g1_set_cpu_port,
 	.set_egress_port = mv88e6095_g1_set_egress_port,
 	.watchdog_ops = &mv88e6097_watchdog_ops,
@@ -4719,7 +4741,7 @@ static const struct mv88e6xxx_ops mv88e6176_ops = {
 	.stats_set_histogram = mv88e6095_g1_stats_set_histogram,
 	.stats_get_sset_count = mv88e6095_stats_get_sset_count,
 	.stats_get_strings = mv88e6095_stats_get_strings,
-	.stats_get_stats = mv88e6095_stats_get_stats,
+	.stats_get_stat = mv88e6095_stats_get_stat,
 	.set_cpu_port = mv88e6095_g1_set_cpu_port,
 	.set_egress_port = mv88e6095_g1_set_egress_port,
 	.watchdog_ops = &mv88e6097_watchdog_ops,
@@ -4771,7 +4793,7 @@ static const struct mv88e6xxx_ops mv88e6185_ops = {
 	.stats_set_histogram = mv88e6095_g1_stats_set_histogram,
 	.stats_get_sset_count = mv88e6095_stats_get_sset_count,
 	.stats_get_strings = mv88e6095_stats_get_strings,
-	.stats_get_stats = mv88e6095_stats_get_stats,
+	.stats_get_stat = mv88e6095_stats_get_stat,
 	.set_cpu_port = mv88e6095_g1_set_cpu_port,
 	.set_egress_port = mv88e6095_g1_set_egress_port,
 	.watchdog_ops = &mv88e6097_watchdog_ops,
@@ -4822,7 +4844,7 @@ static const struct mv88e6xxx_ops mv88e6190_ops = {
 	.stats_set_histogram = mv88e6390_g1_stats_set_histogram,
 	.stats_get_sset_count = mv88e6320_stats_get_sset_count,
 	.stats_get_strings = mv88e6320_stats_get_strings,
-	.stats_get_stats = mv88e6390_stats_get_stats,
+	.stats_get_stat = mv88e6390_stats_get_stat,
 	.set_cpu_port = mv88e6390_g1_set_cpu_port,
 	.set_egress_port = mv88e6390_g1_set_egress_port,
 	.watchdog_ops = &mv88e6390_watchdog_ops,
@@ -4887,7 +4909,7 @@ static const struct mv88e6xxx_ops mv88e6190x_ops = {
 	.stats_set_histogram = mv88e6390_g1_stats_set_histogram,
 	.stats_get_sset_count = mv88e6320_stats_get_sset_count,
 	.stats_get_strings = mv88e6320_stats_get_strings,
-	.stats_get_stats = mv88e6390_stats_get_stats,
+	.stats_get_stat = mv88e6390_stats_get_stat,
 	.set_cpu_port = mv88e6390_g1_set_cpu_port,
 	.set_egress_port = mv88e6390_g1_set_egress_port,
 	.watchdog_ops = &mv88e6390_watchdog_ops,
@@ -4950,7 +4972,7 @@ static const struct mv88e6xxx_ops mv88e6191_ops = {
 	.stats_set_histogram = mv88e6390_g1_stats_set_histogram,
 	.stats_get_sset_count = mv88e6320_stats_get_sset_count,
 	.stats_get_strings = mv88e6320_stats_get_strings,
-	.stats_get_stats = mv88e6390_stats_get_stats,
+	.stats_get_stat = mv88e6390_stats_get_stat,
 	.set_cpu_port = mv88e6390_g1_set_cpu_port,
 	.set_egress_port = mv88e6390_g1_set_egress_port,
 	.watchdog_ops = &mv88e6390_watchdog_ops,
@@ -5016,7 +5038,7 @@ static const struct mv88e6xxx_ops mv88e6240_ops = {
 	.stats_set_histogram = mv88e6095_g1_stats_set_histogram,
 	.stats_get_sset_count = mv88e6095_stats_get_sset_count,
 	.stats_get_strings = mv88e6095_stats_get_strings,
-	.stats_get_stats = mv88e6095_stats_get_stats,
+	.stats_get_stat = mv88e6095_stats_get_stat,
 	.set_cpu_port = mv88e6095_g1_set_cpu_port,
 	.set_egress_port = mv88e6095_g1_set_egress_port,
 	.watchdog_ops = &mv88e6097_watchdog_ops,
@@ -5076,7 +5098,7 @@ static const struct mv88e6xxx_ops mv88e6250_ops = {
 	.stats_set_histogram = mv88e6095_g1_stats_set_histogram,
 	.stats_get_sset_count = mv88e6250_stats_get_sset_count,
 	.stats_get_strings = mv88e6250_stats_get_strings,
-	.stats_get_stats = mv88e6250_stats_get_stats,
+	.stats_get_stat = mv88e6250_stats_get_stat,
 	.set_cpu_port = mv88e6095_g1_set_cpu_port,
 	.set_egress_port = mv88e6095_g1_set_egress_port,
 	.watchdog_ops = &mv88e6250_watchdog_ops,
@@ -5123,7 +5145,7 @@ static const struct mv88e6xxx_ops mv88e6290_ops = {
 	.stats_set_histogram = mv88e6390_g1_stats_set_histogram,
 	.stats_get_sset_count = mv88e6320_stats_get_sset_count,
 	.stats_get_strings = mv88e6320_stats_get_strings,
-	.stats_get_stats = mv88e6390_stats_get_stats,
+	.stats_get_stat = mv88e6390_stats_get_stat,
 	.set_cpu_port = mv88e6390_g1_set_cpu_port,
 	.set_egress_port = mv88e6390_g1_set_egress_port,
 	.watchdog_ops = &mv88e6390_watchdog_ops,
@@ -5189,7 +5211,7 @@ static const struct mv88e6xxx_ops mv88e6320_ops = {
 	.stats_set_histogram = mv88e6095_g1_stats_set_histogram,
 	.stats_get_sset_count = mv88e6320_stats_get_sset_count,
 	.stats_get_strings = mv88e6320_stats_get_strings,
-	.stats_get_stats = mv88e6320_stats_get_stats,
+	.stats_get_stat = mv88e6320_stats_get_stat,
 	.set_cpu_port = mv88e6095_g1_set_cpu_port,
 	.set_egress_port = mv88e6095_g1_set_egress_port,
 	.watchdog_ops = &mv88e6390_watchdog_ops,
@@ -5236,7 +5258,7 @@ static const struct mv88e6xxx_ops mv88e6321_ops = {
 	.stats_set_histogram = mv88e6095_g1_stats_set_histogram,
 	.stats_get_sset_count = mv88e6320_stats_get_sset_count,
 	.stats_get_strings = mv88e6320_stats_get_strings,
-	.stats_get_stats = mv88e6320_stats_get_stats,
+	.stats_get_stat = mv88e6320_stats_get_stat,
 	.set_cpu_port = mv88e6095_g1_set_cpu_port,
 	.set_egress_port = mv88e6095_g1_set_egress_port,
 	.watchdog_ops = &mv88e6390_watchdog_ops,
@@ -5285,7 +5307,7 @@ static const struct mv88e6xxx_ops mv88e6341_ops = {
 	.stats_set_histogram = mv88e6390_g1_stats_set_histogram,
 	.stats_get_sset_count = mv88e6320_stats_get_sset_count,
 	.stats_get_strings = mv88e6320_stats_get_strings,
-	.stats_get_stats = mv88e6390_stats_get_stats,
+	.stats_get_stat = mv88e6390_stats_get_stat,
 	.set_cpu_port = mv88e6390_g1_set_cpu_port,
 	.set_egress_port = mv88e6390_g1_set_egress_port,
 	.watchdog_ops = &mv88e6390_watchdog_ops,
@@ -5350,7 +5372,7 @@ static const struct mv88e6xxx_ops mv88e6350_ops = {
 	.stats_set_histogram = mv88e6095_g1_stats_set_histogram,
 	.stats_get_sset_count = mv88e6095_stats_get_sset_count,
 	.stats_get_strings = mv88e6095_stats_get_strings,
-	.stats_get_stats = mv88e6095_stats_get_stats,
+	.stats_get_stat = mv88e6095_stats_get_stat,
 	.set_cpu_port = mv88e6095_g1_set_cpu_port,
 	.set_egress_port = mv88e6095_g1_set_egress_port,
 	.watchdog_ops = &mv88e6097_watchdog_ops,
@@ -5396,7 +5418,7 @@ static const struct mv88e6xxx_ops mv88e6351_ops = {
 	.stats_set_histogram = mv88e6095_g1_stats_set_histogram,
 	.stats_get_sset_count = mv88e6095_stats_get_sset_count,
 	.stats_get_strings = mv88e6095_stats_get_strings,
-	.stats_get_stats = mv88e6095_stats_get_stats,
+	.stats_get_stat = mv88e6095_stats_get_stat,
 	.set_cpu_port = mv88e6095_g1_set_cpu_port,
 	.set_egress_port = mv88e6095_g1_set_egress_port,
 	.watchdog_ops = &mv88e6097_watchdog_ops,
@@ -5447,7 +5469,7 @@ static const struct mv88e6xxx_ops mv88e6352_ops = {
 	.stats_set_histogram = mv88e6095_g1_stats_set_histogram,
 	.stats_get_sset_count = mv88e6095_stats_get_sset_count,
 	.stats_get_strings = mv88e6095_stats_get_strings,
-	.stats_get_stats = mv88e6095_stats_get_stats,
+	.stats_get_stat = mv88e6095_stats_get_stat,
 	.set_cpu_port = mv88e6095_g1_set_cpu_port,
 	.set_egress_port = mv88e6095_g1_set_egress_port,
 	.watchdog_ops = &mv88e6097_watchdog_ops,
@@ -5516,7 +5538,7 @@ static const struct mv88e6xxx_ops mv88e6390_ops = {
 	.stats_set_histogram = mv88e6390_g1_stats_set_histogram,
 	.stats_get_sset_count = mv88e6320_stats_get_sset_count,
 	.stats_get_strings = mv88e6320_stats_get_strings,
-	.stats_get_stats = mv88e6390_stats_get_stats,
+	.stats_get_stat = mv88e6390_stats_get_stat,
 	.set_cpu_port = mv88e6390_g1_set_cpu_port,
 	.set_egress_port = mv88e6390_g1_set_egress_port,
 	.watchdog_ops = &mv88e6390_watchdog_ops,
@@ -5585,7 +5607,7 @@ static const struct mv88e6xxx_ops mv88e6390x_ops = {
 	.stats_set_histogram = mv88e6390_g1_stats_set_histogram,
 	.stats_get_sset_count = mv88e6320_stats_get_sset_count,
 	.stats_get_strings = mv88e6320_stats_get_strings,
-	.stats_get_stats = mv88e6390_stats_get_stats,
+	.stats_get_stat = mv88e6390_stats_get_stat,
 	.set_cpu_port = mv88e6390_g1_set_cpu_port,
 	.set_egress_port = mv88e6390_g1_set_egress_port,
 	.watchdog_ops = &mv88e6390_watchdog_ops,
@@ -5654,7 +5676,7 @@ static const struct mv88e6xxx_ops mv88e6393x_ops = {
 	.stats_set_histogram = mv88e6390_g1_stats_set_histogram,
 	.stats_get_sset_count = mv88e6320_stats_get_sset_count,
 	.stats_get_strings = mv88e6320_stats_get_strings,
-	.stats_get_stats = mv88e6390_stats_get_stats,
+	.stats_get_stat = mv88e6390_stats_get_stat,
 	/* .set_cpu_port is missing because this family does not support a global
 	 * CPU port, only per port CPU port which is set via
 	 * .port_set_upstream_port method.
diff --git a/drivers/net/dsa/mv88e6xxx/chip.h b/drivers/net/dsa/mv88e6xxx/chip.h
index 0ad34b2d8913..268c97cde8d8 100644
--- a/drivers/net/dsa/mv88e6xxx/chip.h
+++ b/drivers/net/dsa/mv88e6xxx/chip.h
@@ -318,6 +318,17 @@ struct mv88e6xxx_mst {
 	struct mv88e6xxx_stu_entry stu;
 };
 
+#define STATS_TYPE_PORT		BIT(0)
+#define STATS_TYPE_BANK0	BIT(1)
+#define STATS_TYPE_BANK1	BIT(2)
+
+struct mv88e6xxx_hw_stat {
+	char string[ETH_GSTRING_LEN];
+	size_t size;
+	int reg;
+	int type;
+};
+
 struct mv88e6xxx_chip {
 	const struct mv88e6xxx_info *info;
 
@@ -574,8 +585,9 @@ struct mv88e6xxx_ops {
 	/* Return the number of strings describing statistics */
 	int (*stats_get_sset_count)(struct mv88e6xxx_chip *chip);
 	int (*stats_get_strings)(struct mv88e6xxx_chip *chip,  uint8_t *data);
-	int (*stats_get_stats)(struct mv88e6xxx_chip *chip,  int port,
-			       uint64_t *data);
+	int (*stats_get_stat)(struct mv88e6xxx_chip *chip,  int port,
+			      const struct mv88e6xxx_hw_stat *stat,
+			      uint64_t *data);
 	int (*set_cpu_port)(struct mv88e6xxx_chip *chip, int port);
 	int (*set_egress_port)(struct mv88e6xxx_chip *chip,
 			       enum mv88e6xxx_egress_direction direction,
@@ -736,17 +748,6 @@ struct mv88e6xxx_ptp_ops {
 	u32 cc_mult_dem;
 };
 
-#define STATS_TYPE_PORT		BIT(0)
-#define STATS_TYPE_BANK0	BIT(1)
-#define STATS_TYPE_BANK1	BIT(2)
-
-struct mv88e6xxx_hw_stat {
-	char string[ETH_GSTRING_LEN];
-	size_t size;
-	int reg;
-	int type;
-};
-
 static inline bool mv88e6xxx_has_stu(struct mv88e6xxx_chip *chip)
 {
 	return chip->info->max_sid > 0 &&
-- 
2.34.1

