/ {
       config {
               env: environment {
                       /* After the MMC driver has enabled bus power,
                        * the controller seems to sometimes detect a
                        * card removal state , which causes it to
                        * disable power again. This hack re-enables the
                        * bus power in those cases.
                        */
                       bootcmd = "run ixboot";
                       boot_targets = "mmc0";
                       ethprime = "eth0";
                       fdt_addr_r = "0x43f00000";
                       kernel_addr_r = "0x44000000";
                       scriptaddr = "0x48000000";
                       ramdisk_addr_r = "0x4A000000";

		en8811h_fw_part = "0#en8811h_fw";
		en8811h_fw_dm_dir = "EthMD32.dm.bin";
		en8811h_fw_dsp_dir = "EthMD32.DSP.bin";

                       /* This is a development platform, keep
                        * developer mode statically enabled.
                        */
                       ixbtn-devmode = "setenv dev_mode yes; echo Enabled";
                       ixbtn-factory = "echo \"No button available, use bootmenu\"";
               };
       };
};
