=== Dual bridges on one device

ifdef::topdoc[:imagesdir: {topdoc}../../test/case/interfaces/dual_bridge]

==== Description

Verify that it is possible to ping through a bridge to another bridge
via a VETH pair connected to both.

....
 PING -->     br0             br1 10.0.0.2
             /   \              /
PC - target:data  veth0a - veth0b
....

==== Topology

image::topology.svg[Dual bridges on one device topology, align=center, scaledwidth=75%]

==== Sequence

. Set up topology and attach to target DUTs
. Configure two bridges linked and a veth pair
. Verify ping from host:data to 10.0.0.2


