=== Bridge basic

ifdef::topdoc[:imagesdir: {topdoc}../../test/case/interfaces/bridge_basic]

==== Description

Test basic connectivity to a bridge

....

    PING -->                br0 (10.0.0.2)
                            /
    PC -------- target:data

....

==== Topology

image::topology.svg[Bridge basic topology, align=center, scaledwidth=75%]

==== Sequence

. Set up topology and attach to target DUT
. Configure single bridge with a single physical port, bridge @ IP 10.0.0.2
. Verify ping 10.0.0.2 is possible from host:data


