// SPDX-License-Identifier: (GPL-2.0 OR MIT)
/*
 * Copyright (C) 2021 MediaTek Inc.
 * Author: Sam.Shih <sam.shih@mediatek.com>
 */

/*
This is copied from linux where it is an overlay, unfortunatly it is not
possible to use dtbo in sysboot unless present in syslinux.conf
*/
&{/soc/mmc@11230000} {
        bus-width = <8>;
        max-frequency = <200000000>;
        cap-mmc-highspeed;
        mmc-hs200-1_8v;
        mmc-hs400-1_8v;
        hs400-ds-delay = <0x14014>;
        non-removable;
        no-sd;
        no-sdio;
        status = "okay";
};
