=== LACP Aggregate w/ Degraded Link

ifdef::topdoc[:imagesdir: {topdoc}../../test/case/interfaces/lag_failure]

==== Description

Verify communication over an LACP link aggregate when individual member
links stop forwarding traffic, without carrier loss.

.Logical network setup, link breakers (lb1 & lb2) here managed by host PC
image::lag-failure.svg[align=center, scaledwidth=75%]

The host verifies connectivity with dut2 via dut1 over the aggregate for
each failure mode step using the `mon` interface.

==== Topology

image::topology.svg[LACP Aggregate w/ Degraded Link topology, align=center, scaledwidth=75%]

==== Sequence

. Set up topology and attach to target DUTs
. Set up link aggregate, lag0, between dut1 and dut2
. Initial connectivity check ...
. Verify failure modes


