Mode                : Client

[7mADDRESS      MODE    STATE      STRATUM  POLL[0m
192.168.1.1  server  candidate        1   64s
192.168.2.1  server  candidate        1   64s
192.168.3.1  server  selected         1   64s
