[7m⚑ INTERFACE       PROTOCOL   STATE       DATA                                     [0m
  lo              loopback   [32mUP          [39m
                  ipv4                   127.0.0.1/8 (static)
                  ipv6                   ::1/128 (static)
  br0             bridge     [33m            [39mvlan:1u pvid:1                           
  │               ethernet   [32mUP          [39m00:a0:85:00:03:00                        
  │               ipv4                   169.254.1.1/16 (random)
  │               ipv6                   fe80::2a0:85ff:fe00:300/64 (link-layer)
  ├ e3            bridge     [32mFORWARDING  [39mvlan:1u pvid:1                           
  ├ e4            bridge     [32mFORWARDING  [39mvlan:1u pvid:1                           
  ├ veth0b        bridge     [32mFORWARDING  [39mvlan:1u pvid:1                           
  └ veth2b        bridge     [32mFORWARDING  [39mvlan:1u pvid:1                           
  br1             bridge     [33m            [39m
  │               ethernet   [32mUP          [39m00:a0:85:00:03:00                        
  ├ veth1b        bridge     [32mFORWARDING  [39mvlan:6u pvid:6                           
  └ veth3b        bridge     [32mFORWARDING  [39m
  e1              ethernet   [32mUP          [39m00:a0:85:00:03:01                        
                  ipv6                   fe80::2a0:85ff:fe00:301/64 (link-layer)
  e2              ethernet   [32mUP          [39m00:a0:85:00:03:02                        
                  ipv6                   fe80::2a0:85ff:fe00:302/64 (link-layer)
  e3.8            ethernet   [32mUP          [39m00:a0:85:00:03:03                        
  │               ipv4                   10.1.1.1/32 (static)
  └ e3            ethernet   [32mUP          [39m00:a0:85:00:03:03                        
  e4.8            ethernet   [32mUP          [39m00:a0:85:00:03:04                        
  │               ipv4                   10.1.1.1/32 (static)
  └ e4            ethernet   [32mUP          [39m00:a0:85:00:03:04                        
  e5              ethernet   [32mUP          [39m00:a0:85:00:03:05                        
                  ipv6                   fe80::2a0:85ff:fe00:305/64 (link-layer)
  e6              ethernet   [32mUP          [39m00:a0:85:00:03:06                        
                  ipv4                   10.1.1.101/24 (static)
                  ipv6                   fe80::2a0:85ff:fe00:306/64 (link-layer)
  e7              ethernet   [32mUP          [39m00:a0:85:00:03:07                        
                  ipv6                   fe80::2a0:85ff:fe00:307/64 (link-layer)
  [100mveth0a          container              container-A                              [0m
  veth0b          veth       [32mUP          [39me6:19:75:86:80:dd                        
  [100mveth1a          container              container-A                              [0m
  veth1b          veth       [32mUP          [39m3e:67:0f:15:24:14                        
  [100mveth2a          container              container-B                              [0m
  veth2b          veth       [32mUP          [39mb2:fa:30:63:98:f0                        
  [100mveth3a          container              container-B                              [0m
  veth3b          veth       [32mUP          [39mb2:1c:fa:a7:45:eb                        
