=== DHCP Server Static Host

ifdef::topdoc[:imagesdir: {topdoc}../../test/case/dhcp/server_host]

==== Description

Verify DHCP server can hand out static host leases based on client-id,
both hexadecimal and a very long string, ensuring no pool address is
handed out instead.

==== Topology

image::topology.svg[DHCP Server Static Host topology, align=center, scaledwidth=75%]

==== Sequence

. Set up topology and attach to client and server DUTs
. Configure DHCP client and server DUTs
. Verify DHCP client1 static lease
. Verify client1 hostname has *not* changed
. Verify DHCP client1 has default route via option 121
. Verify DHCP client2 static lease
. Verify client2 hostname has changed
. Verify DHCP client2 has default gateway


