From 5a530e4eebf64887fd6b449dd45df04eccd07cad Mon Sep 17 00:00:00 2001
From: Joachim Wiberg <troglobit@gmail.com>
Date: Thu, 12 Feb 2026 10:00:02 +0100
Subject: [PATCH 4/7] arm: dts: at91: sama7g5ek supports high-speed on mmc0
 (eMMC)
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit
Organization: Wires

- eMMC high-speed timing is supported
- eMMC hardware reset is supported

Tested on sama7g5ek rev 5.

Signed-off-by: Joachim Wiberg <troglobit@gmail.com>
Signed-off-by: Mattias Walström <lazzer@gmail.com>
---
 arch/arm/dts/at91-sama7g5ek.dts | 2 ++
 1 file changed, 2 insertions(+)

diff --git a/arch/arm/dts/at91-sama7g5ek.dts b/arch/arm/dts/at91-sama7g5ek.dts
index 5bbbdd8ed76..d2d16bd5f1f 100644
--- a/arch/arm/dts/at91-sama7g5ek.dts
+++ b/arch/arm/dts/at91-sama7g5ek.dts
@@ -776,6 +776,8 @@
 &sdmmc0 {
 	bus-width = <8>;
 	non-removable;
+	cap-mmc-highspeed;
+	cap-mmc-hw-reset;
 	pinctrl-names = "default";
 	pinctrl-0 = <&pinctrl_sdmmc0_default>;
 	status = "okay";
-- 
2.43.0

